# Changing the Intermediate Pad (see figure A)

An intermediate pad (14) must always be used when working with the soft sanding pad (part of standard items included).

To remove the intermediate pad (14), lift it from the side and pull it off the sanding pad (16).

Remove dirt and dust from the sanding pad (16), e.g. with a paintbrush, before attaching a new intermediate pad.

The surface of the sanding pad (16) is fitted with a hook-and-loop fastening, allowing intermediate pads to be secured quickly and easily.

Press the intermediate pad (14) firmly against the underside of the sanding pad (16).

To ensure optimum dust extraction, make sure that the punched holes in the intermediate pad (14) are aligned with the drilled holes in the sanding pad (16).