# Changing the Sanding Pad (see figure B)

Note: Replace damaged sanding pads (16) immediately.

Pull off the sanding sheet (13) and the intermediate pad (14). Unscrew the screw (15) completely and remove the sanding pad (16). Attach the new sanding pad (16) and retighten the screw.

Note: When attaching the sanding pad, make sure that the teeth of the catch mate with the recesses in the sanding pad.

Note: Damaged sanding pads must only be replaced by an after-sales service centre authorised to work with Bosch power tools.