# Technical Data

Angle Grinder |  | GWS 20-125 SB | GWS 20-125 TSB
--- | --- | --- | ---
Article number |  | ‎3 601 GD5 0..‎ | ‎3 601 GD5 2..‎
Rated power input | W | 2000 | 2000
Power output | W | 1400 | 1400
Rated no-load speedA) | min-1 | 10500 | 9700
Speed adjustment range | min-1 | 2800–10500 | 2400–9700
Max. grinding disc diameter/rubber sanding pad diameter | mm | 125 | 125
Grinding spindle thread |  | M 14 | M 14
Max. thread length of grinding spindle | mm | 21 | 21
Speed preselection |  | ● | ●
Constant electronic control |  | ● | ●
Overload protection |  | ● | ●
Restart protection |  | ● | ●
Soft start |  | ● | ●
Kickback stop |  | ● | ●
Run-out brake |  | ● | ●
Drop Control |  | ● | ●
Status indicator (LED) |  | ● | ●
WeightB)C) | kg | 2.3–2.7 | 2.3–2.7
Protection class |  | / II | / II

A)

  Rated no-load speed for the selection of appropriate application tools in accordance with EN IEC 62841-2-3. The actual no-load speed must not exceed the rated no-load speed and is therefore lower.

B)

  Depends on protective guard ((11), (10), (12)) and auxiliary handle ((7), (8)) in use

C)

  Weight without mains connection cable and without mains plug

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.