# Operation

- Do not load the power tool so heavily that it comes to a stop.

- Pull the plug out of the socket before carrying out any work on the power tool.

- Exercise caution when cutting slots in structural walls; see the "Information on structural design" section.

- Clamp the workpiece if it is not secure under its own weight.

- If the power tool has been subjected to a heavy load, continue to run it at no-load for several minutes to cool down the accessory.

- Do not use the power tool with a cut-off stand.

- Do not touch grinding and cutting discs until they have cooled down. The discs can become very hot while working.

Working advice
Start-Up