# Technical data

Angle Grinder |  | GWS 20-230 P | GWS 20-230 J
--- | --- | --- | ---
Article number |  | ‎3 601 HC1 1..‎ | ‎3 601 HC1 3..‎
Rated power input | W | 2000 | 2000
Rated no-load speedA) | min–1 | 6500 | 6500
Max. grinding disc diameter/rubber sanding pad diameter | mm | 230 | 230
Grinding spindle thread |  | M 14 | M 14
Max. thread length of grinding spindle | mm | 25 | 25
Restart protection |  | – | ●
Soft start |  | – | ●
WeightB)C) | kg | 5.4–8.8 | 5.4–8.8
Protection class |  | / II | / II

A)

  Rated no-load speed for the selection of appropriate application tools in accordance with EN IEC 62841-2-3. The actual no-load speed must not exceed the rated no-load speed and is therefore lower.

B)

  Depends on protective guard ((7), (6), (8)), auxiliary handle ((4), (3)) and extraction guard (24) in use

C)

  Weight without mains connection cable and without mains plug

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

## Notes on mains connection requirements for GWS 20-230 P:

The appliance meets IEC 61000-3-11 requirements and is subject to conditional connection. The appliance can lead to occasional voltage fluctuations under unfavorable power conditions. The impedance of this appliance is set as Zactual = 0.18 Ω. The user must make sure, that the connection point, with the impedance Zmax, on which the appliance shall be plugged in meets the impedance requirement: Zactual ≥ Zmax. If Zmax is unknown, determine Zmax in consultation with the network supplier or supply authority.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.

Angle Grinder |  | GWS 22-180 P GWS 2200 | GWS 22-230 P GWS 2200 | GWS 22-180 J GWS 2200 | GWS 22-230 J GWS 2200
--- | --- | --- | --- | --- | ---
Article number |  | ‎3 601 HC0 1..‎ | ‎3 601 HC1 1..‎ | ‎3 601 HC0 3..‎ | ‎3 601 HC1 3..‎
Rated power input | W | 2200 | 2200 | 2200 | 2200
Rated no-load speedA) | min–1 | 8500 | 6500 | 8500 | 6500
Max. grinding disc diameter/rubber sanding pad diameter | mm | 180 | 230 | 180 | 230
Grinding spindle thread |  | M 14 | M 14 | M 14 | M 14
Max. thread length of grinding spindle | mm | 25 | 25 | 25 | 25
Restart protection |  | – | – | ● | ●
Soft start |  | – | – | ● | ●
WeightB)C) | kg | 5.2–7.8 | 5.4–8.8 | 5.2–7.8 | 5.4–8.8
Protection class |  | / II | / II | / II | / II

A)

  Rated no-load speed for the selection of appropriate application tools in accordance with EN IEC 62841-2-3. The actual no-load speed is lower.

B)

  Depends on protective guard ((7), (6), (8)), auxiliary handle ((4), (3)) and extraction guard (24) in use

C)

  Weight without mains connection cable and without mains plug

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

## Notes on mains connection requirements for GWS 22-180 P, GWS 22-230 P and GWS 2200:

The appliance meets IEC 61000-3-11 requirements and is subject to conditional connection. The appliance can lead to occasional voltage fluctuations under unfavorable power conditions. The impedance of this appliance is set as Zactual = 0.18 Ω. The user must make sure, that the connection point, with the impedance Zmax, on which the appliance shall be plugged in meets the impedance requirement: Zactual ≥ Zmax. If Zmax is unknown, determine Zmax in consultation with the network supplier or supply authority.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.