# Technical data

Angle Grinder |  | GWS 2000 J | GWS 2000 P | GWS 2200 J | GWS 2200 P | GWS 2400 J | GWS 2400 P
--- | --- | --- | --- | --- | --- | --- | ---
Article number |  | ‎3 601 HF2 0..‎‎‎‎ | ‎3 601 HF2 1..‎‎‎‎ | ‎3 601 HF4 0..‎‎‎‎ | ‎3 601 HF4 1..‎‎‎‎ | ‎3 601 HF4 2..‎‎‎‎ | ‎3 601 HF4 3..‎‎‎‎
Rated power input | W | 2000 | 2000 | 2200 | 2200 | 2400 | 2400
Rated speed | min−1 | 6500 | 6500 | 6500 | 6500 | 6500 | 6500
Max. grinding disc diameter | mm | 230 | 230 | 230 | 230 | 230 | 230
Grinding spindle thread |  | M14 | M14 | M14 | M14 | M14 | M14
Max. thread length of grinding spindle | mm | 25 | 25 | 25 | 25 | 25 | 25
Restart protection |  | ● | – | ● | – | ● | –
Soft start |  | ● | – | ● | – | ● | –
Weight according to EPTA-Procedure 01:2014
with low-vibration auxiliary handle | kg | 5.2 | 5.1 | 5.5 | 5.4 | 5.5 | 5.4
with standard auxiliary handle | kg | 5.1 | 5.0 | 5.4 | 5.3 | 5.4 | 5.3
Protection class |  | /II | /II | /II | /II | /II | /II

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

## Notes on mains connection requirements for GWS 2000 P/GWS 2200 P/GWS 2400 P:

The appliance meets IEC 61000-3-11 requirements and is subject to conditional connection. The appliance can lead to occasional voltage fluctuations under unfavorable power conditions. The impedance of this appliance is set as Zactual = 0.18 Ω. The user must make sure, that the connection point, with the impedance Zmax, on which the appliance shall be plugged in meets the impedance requirement: Zactual ≥ Zmax. If Zmax is unknown, determine Zmax in consultation with the network supplier or supply authority.