# Approved abrasive tools

You can use all the abrasive tools mentioned in these operating instructions.

The permissible speed [min-1] or the circumferential speed [m/s] of the abrasive tools used must at least match the values given in the table.

It is therefore important to observe the permissible rotational/circumferential speed on the label of the abrasive tool.

| Max. [mm] | [mm] |  |
--- | --- | --- | --- | ---
| D | b | d | [min-1] | [m/s]
| 230 | 8 | 22.2 | 6500 | 80
| 180 | – | – | 6500 | 80
| 100 | 30 | M14 | 8500 | 45