# Fitting Protective Equipment

- Pull the plug out of the socket before carrying out any work on the power tool.

Note: If the grinding disc breaks during operation or the holding fixtures on the protective guard/power tool become damaged, the power tool must be sent to the after-sales service immediately; see the "After-Sales Service and Application Service" section for addresses.

##

Place the protective guard (6) on the spindle collar. Adjust the position of the protective guard (6) to the requirements of the operation and lock the protective guard (6) with the locking screw (7).

- Adjust the protective guard (6) such that sparking in the direction of the operator is prevented.

##

- Always use the protective guard for cutting (14) when cutting with bonded abrasives.

- Provide sufficient dust extraction when cutting stone.

The protective guard for cutting (14) is fitted in the same way as the protective guard for grinding (6).

##

Observe the operating instructions of the extraction guard when fitting the extraction guard for cutting with a cutting guide (23).

##

- Do not operate your power tool without the side handle (3).

Screw the side handle (3) on the left or right of the machine head depending on how your are working.

##

- Always fit the hand guard (16) when working with the rubber sanding plate (18) or with the cup brush/disc brush/flap disc.

Attach the hand guard (16) to the side handle (3).