# Technical Data

Angle grinder |  | GWS 30-180 B | GWS 30-230 B | GWS 30-180 PB | GWS 30-230 PB | GWS 30-230 B
--- | --- | --- | --- | --- | --- | ---
Article number |  | ‎3 601 HG0 0..‎ | ‎3 601 HG1 0..‎ | ‎3 601 HG0 1..‎ | ‎3 601 HG1 1..‎ | ‎3 601 HG1 0..‎
Rated power input | W | 2800 | 2800 | 2800 | 2800 | 2200
Rated no-load speedA) | min–1 | 8500 | 6500 | 8500 | 6500 | 6500
Max. grinding disc diameter/rubber backing pad diameter | mm | 180 | 230 | 180 | 230 | 230
Grinding spindle thread |  | M 14 | M 14 | M 14 | M 14 | M 14
Max. thread length of grinding spindle | mm | 25 | 25 | 25 | 25 | 25
KickBack Control |  | ● | ● | ● | ● | ●
Restart protection |  | ● | ● | ● | ● | ●
Soft start |  | ● | ● | ● | ● | ●
Run-out brake |  | ● | ● | ● | ● | ●
Status indicator (LED) |  | ● | ● | ● | ● | ●
PROtection switch |  | – | – | ● | ● | –
WeightB)C) | kg | 5,7–7,5 | 5,9–8,4 | 5,7–7,5 | 5,9–8,4 | 5,9–8,4
Protection class |  | / II | / II | / II | / II | / II

A)

  Rated no-load speed for the selection of appropriate application tools in accordance with EN IEC 62841-2-3. The actual no-load speed must not exceed the rated no-load speed and is therefore lower.

B)

  Depends on protective guard ((17), (18), (8), (9), (19)), auxiliary handle ((5), (6)) and extraction guard (34) in use

C)

  Weight without mains connection cable and without mains plug

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.