# Technical data

Cordless multi-cutter | GOP 185‑LI
--- | ---
Article number |  | ‎3 601 HG2 0..‎‎‎‎
Rated voltage | V= | 18
No-load speed n₀ | min−1 | 10000–20000
Oscillation angle on left/right | ° | 1.7
Weight according to ‌EPTA-Procedure 01:2014 | kg | 1.5−2.6A)
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationB) and during storage | °C | −20 to +50
Recommended rechargeable batteries |  | GBA 18V… ProCORE18V…
Recommended chargers |  | GAL 18… GAX 18… GAL 36…

A)

  Depends on battery in use

B)

  Limited performance at temperatures < 0 °C

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.