# Assembly

- Pull the plug out of the socket before cleaning or performing maintenance on the vacuum cleaner, making tool adjustments, changing accessories or putting away the vacuum cleaner. This safety measure prevents the vacuum cleaner from being started accidentally.

Fitting the Extraction Accessories
Fitting the holder for the vacuum hose
Fitting the vacuum hose
Inserting/removing the disposal bag or dust bag (dry extraction)