# Technical data

Wet/dry dust extractor |  | GAS 20 L SFC
--- | --- | ---
Article number |  | ‎3 601 J7B 1..‎‎‎‎
Rated voltage | V | 220–240
Rated power input | W | 1200
Frequency | Hz | 50–60
Container volume (gross/net) | l | 19/15
Net volume (liquid) | l | 11.5
Dust bag volume | l | 7.5
Max. vacuumA)
Dust extractor | hPa | 202
Turbine | hPa | 215
Max. volume flow rateA)
Dust extractor | l/s m³/s | 31.5 0.0315
Turbine | l/s m³/s | 62 0.062
Max. suction power | W | 245
Area of pleated filter | m² | 0.28
Dust class |  | L
Weight according to EPTA-Procedure 01:2014 | kg | 6.4
Protection class |  | /I
Dust extractor protection rating |  | IPX4
Mains plug Switzerland protection rating |  | IP55

A)

  Measured using a vacuum hose 3 m long and 35 mm in diameter

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.

Automatic start/stopA)
| Rated voltage | Maximum power | Minimum power
--- | --- | --- | ---
EU | 230 V | 2000 W | 100 W
FR | 230 V | 2000 W | 100 W
UK | 230 V | 1700 W | 100 W
CH | 230 V | 1100 W | 100 W
DK | 230 V | 1100 W | 100 W

A)

  Permitted connected load of the connected power tool (country-specific)