# Technical Data

Straight grinder |  | GGS 18V-20
--- | --- | ---
Article number |  | ‎3 601 JB5 4..‎
Rated voltage | V= | 18
Rated speedA) | min-1 | 24,000
Max. collet diameter | mm | 8
Spanner flat on the
Clamping nut | mm | 19
Grinding spindle | mm | 19
Grinding tool diameter, max. | mm | 50
Weight according to EPTA-Procedure 01:2014B) | kg | 1.5–2.5
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V...
Recommended chargers |  | GAL 18… GAX 18… GAL 36…

A)

  Rated no-load speed for the selection of appropriate grinding tools in accordance with EN 60745. The actual speed is lower for safety reasons.

B)

  Depends on battery in use

C)

  Limited performance at temperatures < 0 °C

Technical data determined with rechargeable battery ProCORE18V 8.0Ah.