# Storage and transport (see figure L)

- Wrap the power cable around the cable holder (13).
- Insert the accessory into the holders provided for it: Suction tubes (29) into the holders (15), crevice nozzle (25) into the holder (16), floor nozzle (28) into the holder (17).
- Open the elastic bands of the vacuum hose holder (4) and wrap the vacuum hose (21) around the top part of the dust extractor in the holder (4).
  Hook the elastic bands back in.
- Click the L-Boxx on to the adapters (7).
- Before transporting the dust extractor, remove any full disposal bags/dust bags and empty any liquids that have been absorbed, in order to avoid placing unnecessary strain on the back and prevent injury.
  Only ever carry the dust extractor by the carrying handle (6).
- Store the dust extractor in a dry room and secure it so that it cannot be used by unauthorised persons.
- Put the castor brake (11) down to hold the castors (12) in place.