# Inserting/removing the disposal bag or dust bag (dry extraction) (see figures E1–E2)

For dry vacuuming, you can insert a disposal bag (23) or a dust bag (accessory) into the container (1). This makes the dust easier to dispose of.

Note: If using a paper filter bag, you must make sure that semi-automatic filter cleaning (SFC+) is switched off; you should also do the same if using a fleece filter bag see Semi-automatic filter cleaning (see figure I).

##

- Open the catches (9) and remove the top part of the vacuum cleaner (8).

- Insert the disposal bag (23) into the container (1) with the inlet facing forwards.
- Pull the inlet over the connection flange and all the way into the recess of the connection flange.
- Make sure that the disposal bag (23) touches all the inside walls of the container (1).
- Fold the rest of the disposal bag (23) over the edge of the container (1).

- Put the top part of the vacuum cleaner (8) on and close the catches (9).

##

- Open the catches (9) and remove the top part of the vacuum cleaner (8).

- Pull the full disposal bag (23) backwards out of the connection flange.
- Carefully take the disposal bag (23) out of the container (1) without damaging it.
  When doing so, make sure that the disposal bag does not scrape against the connection flange or other sharp objects.
- Remove the adhesive strip cover and tape up the disposal bag.
  Then tie up the disposal bag (23) below the inlet using the adhesive strip cover that has been removed.

##

- Open the catches (9) and remove the top part of the vacuum cleaner (8).

- Pull the full dust bag backwards out of the connection flange. Close the opening in the dust bag by turning down the top. Take the closed dust bag out of the container (1).
- Place the new dust bag over the vacuum cleaner's connection flange. Make sure that the entire length of the dust bag touches the inside wall of the container (1).

- Put the top part of the vacuum cleaner (8) on and close the catches (9).