# Technical data

Wet/dry dust extractor |  | GAS 35 L SFC+
--- | --- | ---
Article number |  | ‎‎3 601 JC3 0..‎‎‎
Rated power input | W | 1200
Frequency | Hz | 50–60
Container volume (gross) | l | 35
Net volume (liquid) | l | 19
Dust bag volume | l | 19
Max. vacuumA)
Dust extractor | hPa | 230
Turbine | hPa | 254
Max. flow rateA)
Dust extractor | l/s m³/s m³/h | 36 0.036 129.6
Turbine | l/s m³/s m³/h | 74 0.074 266.4
Max. suction power | W | 1380
Area of pleated filter | m² | 0.615
Dust class |  | L
WeightB) | kg | 11.6
Protection class |  | /I
Dust extractor protection rating |  | IPX4
Mains plug Switzerland protection rating |  | IP55

A)

  Measured using a vacuum hose 3 m long and 35 mm in diameter

B)

  Weight without mains connection cable and without mains plug

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.

Automatic start/stop
Rated voltage | Maximum power | Minimum power
--- | --- | ---
230 V | 2200 W | 100 W

Permitted connected load of the connected power tool.
These values can differ for other country-specific models. Please take note of the information on the socket of the dust extractor.