# Technical data

Wet/dry dust extractor |  | GAS 35 L AFC
--- | --- | ---
Article number |  | ‎3 601 JC3 2..‎
Rated voltage | V | 220–240
Rated power input | W | 1,200
Frequency | Hz | 50–60
Container volume (gross) | l | 35
Net volume (liquid) | l | 19
Dust bag volume | l | 19
Max. vacuumA)
Dust extractor | kPa | 23
Turbine | kPa | 25.4
Max. flow rateA)
Dust extractor | l/s m³/s | 36 0.036
Turbine | l/s m³/s | 74 0.074
Max. suction power | W | 1,380
Area of pleated filter | m² | 0.615
Dust class |  | L
Weight according to EPTA-Procedure 01:2014 | kg | 12.2
Protection class |  | /I
Protection rating |  | IPX4

A)

  Measured using a vacuum hose 3 m long and 35 mm in diameter

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Automatic start/stop
Rated voltage | Maximum power | Minimum power
--- | --- | ---
230 V | 2200 W | 100 W

Permitted connected load of the connected power tool.
These values can differ for other country-specific models. Please take note of the information on the socket of the dust extractor.