# Noise/Vibration Information

Noise emission values determined according to EN 60335-2-69.

Typically the A-weighted sound pressure level of the dust extractor is 70 dB(A). Uncertainty K = 3 dB. The noise level when working can exceed 80 dB(A).

Wear hearing protection

Total vibration values ah (triax vector sum) and uncertainty K determined according to EN 60335-2-69: ah<2.5 m/s2, K = 1.5 m/s2.