# Technical data

Cordless dry vacuum cleaner | GAS 18V-1
--- | ---
Article number |  | ‎3 601 JC6 2..‎‎‎‎
Container volume (gross) | l | 0.7
Max. vacuumA) | kPa | 6
Max. flow rateA) | l/s | 10
Weight according to EPTA-Procedure 01:2014 | kg | 1.7–2.3A)
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationB) and during storage | °C | –20 to +50
Compatible rechargeable batteries |  | GBA 18V… ProCORE18V…
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V... ≤ 8 Ah
Recommended chargers |  | GAL 18… GAX 18… GAL 36…

A)

  Depends on battery in use

B)

  Limited performance at temperatures < 0 °C