# Technical data

Orbital Sander |  | GSS 18V-10
--- | --- | ---
Article number |  | 3 601 JD0 2..
Rated voltage | V= | 18
No-load speedA) | min–1 | 11,000
No-load orbital stroke rateA) | min–1 | 22,000
Sanding sheet surface | cm2 | 114.7
Orbit diameter | mm | 1.6
Dimensions | mm | 199.5 x 113 x 141
Weight | kg | 1.4–2.4
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationB) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V...
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 4.0Ah

B)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.