# Technical Data

Cordless impact Screwdriver |  | GDR 18V-200 C | GDX 18V-200 C | GDS 18V-200 C
--- | --- | --- | --- | ---
Article number |  | 3 601 JG4 1.. | 3 601 JG4 2.. | 3 601 JG4 3..
Rated voltage | V= | 18 | 18 | 18
No-load speedA)
Setting 1 | min–1 | 0–1100 | 0–1100 | 0–1100
Setting 2 | min–1 | 0–2300 | 0–2300 | 0–2300
Setting 3 | min–1 | 0–3400 | 0–3400 | 0–3400
Impact rateA)
Setting 1 | min–1 | 0–2300 | 0–2300 | 0–2300
Setting 2 | min–1 | 0–3400 | 0–3400 | 0–3400
Setting 3 | min–1 | 0–4000 | 0–4200 | 0–4200
Max. torque | Nm | 200 | 200 | 200
Machine screw diameter | mm | M6–M16 | M6–M16 | M6–M16
Tool holder |  | ¼" internal hexagon | ¼" internal hexagon/ ∎ ½" | ∎ ½"
Weight | kg | 1.1–2.5 | 1.2–2.5 | 1.1–2.5
Data transfer
Bluetooth®B) |  | Bluetooth® 4.1 (Low Energy) | Bluetooth® 4.1 (Low Energy) | Bluetooth® 4.1 (Low Energy)
Signal interval | s | 8 | 8 | 8
Max. signal rangeC) | m | 30 | 30 | 30
Frequency range used | MHz | 2402–2480 | 2402–2480 | 2402–2480
Output power | mW | < 1 | < 1 | < 1
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35 | 0 to +35
Permitted ambient temperature during operationD) and during storage | °C | –20 to +50 | –20 to +50 | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V... | GBA 18V... ProCORE18V... | GBA 18V... ProCORE18V...
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36... | GAL 18... GAX 18... GAL 36... | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 5.0Ah

B)

  The mobile devices must be compatible with Bluetooth® Low Energy devices (version 4.1) and support the Generic Access Profile (GAP).

C)

  The signal range may vary greatly depending on external conditions, including the receiving device used. The Bluetooth® range may be significantly weaker inside closed rooms and through metallic barriers (e.g. walls, shelving units, cases, etc.).

D)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.