# Technical Data

Cordless Impact Wrench |  | GDR 18V-200 | GDX 18V-200 | GDS 18V-200
--- | --- | --- | --- | ---
Article number |  | ‎3 601 JJ2 1..‎ | ‎3 601 JJ2 2..‎ | ‎3 601 JJ2 3..‎
Rated voltage | V= | 18 | 18 | 18
No-load speedA) | min–1 | 0–3400 | 0–3400 | 0–3400
Impact rateA) | min–1 | 0–4000 | 0–4200 | 0–4200
Max. torqueA) | Nm | 200 | 200 | 200
Machine screw diameter | mm | M6–M16 | M6–M16 | M6–M16
Tool holder |  | ¼" internal hexagon | ¼" internal hexagon/ ∎ ½" | ∎ ½"
WeightB) | kg | 1.1–2.5 | 1.1–2.5 | 1.1–2.5
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35 | 0 to +35
Permitted ambient temperature during operation and during storage | °C | –20 to +50 | –20 to +50 | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V... | GBA 18V... ProCORE18V... | GBA 18V... ProCORE18V...
Recommended battery chargers |  | GAX 18… GAL 18… GAL 36… | GAX 18… GAL 18… GAL 36… | GAX 18… GAL 18… GAL 36…

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 5.0Ah

B)

  Depending on battery in use

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.