# Technical Data

Cordless Impact Screwdriver |  | GDS 18V-750 C
--- | --- | ---
Article number |  | ‎‎‎‎‎‎‎3 601 JL9 0..‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎‎
Rated voltage | V= | 18
No-load speedA)
Setting 1 | min–1 | 800
Setting 2 | min–1 | 1500
Setting 3 | min–1 | 2400
Impact rateA)
Setting 1 | min–1 | 1500
Setting 2 | min–1 | 2300
Setting 3 | min–1 | 3000
TorqueA)
Setting 1 | Nm | 270
Setting 2 | Nm | 380
Setting 3 | Nm | 750
Max. tightening torqueA) | Nm | 750
Max. loosening torqueA) | Nm | 1000
Machine screw diameter | mm | M12–M22
Tool holder |  | ∎ ½"
Weight | kg | 2.1–3.1
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operation and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V...
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36...
Coin cell | Type | CR 2032
Data transfer
Bluetooth®B) |  | Bluetooth® 4.1 (Low Energy)
Signal interval | s | 8
Max. signal rangeC) | m | 30

A)

  Measured at 20–25 °C with rechargeable battery ProCORE18V 8.0Ah

B)

  The mobile devices must be compatible with Bluetooth® Low Energy devices (version 4.1) and support the Generic Access Profile (GAP).

C)

  The signal range may vary greatly depending on external conditions, including the receiving device used. The Bluetooth® range may be significantly weaker inside closed rooms and through metallic barriers (e.g. walls, shelving units, cases, etc.).

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.