# Noise/Vibration Information

Noise emission values determined according to EN 60335‑2‑69.

Typically the A-weighted sound pressure level of the dust extractor is 73 dB(A). Uncertainty K = 2 dB. The noise level when working can exceed the volume stated. Wear hearing protection!

Vibration total values ah (triax vector sum) and uncertainty K determined according to EN 60335‑2‑69:
ah < 2.5 m/s2, K = 1.5 m/s2.