# Fitting the vacuuming accessories (see figure A)

The vacuum hose (29) has a clip system that can be used to connect vacuuming accessories (combi power tool adapter (25), curved nozzle (31), combi brush nozzle (24)).

##

- Push the curved nozzle (31) onto the vacuum hose (29) until you hear both snap fasteners (35) on the vacuum hose engage.
- To remove the adapter, press the snap fasteners (35) inwards and pull apart the components.

##

- If required, place the suction tubes (30) firmly inside one another and then attach them firmly to the curved nozzle (31).
- Attach the floor nozzle (23) firmly to the suction tube (30) or the curved nozzle (31).

##

The combi power tool adapter (25) consists of the PowerTool adapter (front part) (36) and the PowerTool adapter (rear part) (37).

The combi power tool adapter (25) is compatible with Bosch power tools.

With an inner diameter of 38.5 mm and an outer diameter of 45 mm, the PowerTool adapter (rear part) (37) can be used for power tools manufactured by other brands.

Place the PowerTool adapter (front part) (36) on the PowerTool adapter (rear part) (37) and connect both adapters by twisting them in opposite directions (see figure B).

Push the combi power tool adapter (25) onto the vacuum hose (29) until you hear both push buttons (35) on the vacuum hose click into place.

To remove the adapter, press the push buttons (35) inwards and pull the combi power tool adapter out of the vacuum hose.

To separate the two adapters, loosen the connection by twisting in opposite directions and pulling the adapters apart.

##

Push the combi brush nozzle (24) onto the vacuum hose (29) until you hear both push buttons (35) on the vacuum hose click into place.

To remove the adapter, press the snap fasteners (35) inwards and pull apart the components.

##

You can use the combi brush nozzle (24) as a crevice nozzle or brush.

Press the release button (38) and push the brush forwards to use the combi brush nozzle (24) as a brush.

Press the release button (38) and pull the brush backwards to use the combi brush nozzle (24) as a crevice nozzle.