# Installing the Retractable Guide Handle (Accessory) (see figures J–K)

Note: The retractable guide handle cannot be removed. When assembling, ensure that the guide handle is aligned correctly.

Before inserting the guide handle (42), align it using the R (right) and L (left) markings.

Insert the guide handle (42) into the guide rails (20).

Press the guide handle (42) down to the stop line until the guide handle audibly clicks into place.

Press the snap fastener (41) to change the length of the guide handle (42).