# Inserting/removing the plastic bag (dry extraction) (see figure F)

Open both catches (15) and remove the top part of the dust extractor (12).

For dry extraction, insert a plastic bag (32) into the container (1).

Insert the plastic bag (32) into the container (1) with the inlet facing upwards.

Make sure that the plastic bag (32) touches all the inside walls of the container (1).

Fold the rest of the plastic bag (32) over the edge of the container (1). Make sure that the stop line of the plastic bag is positioned at the edge of the container and the air passage openings (33) are still in the container.

Put the top part of the vacuum cleaner (12) back on and close the vacuum cleaner using the catches (15).

- Ensure that the dust extractor is always properly closed.

Seal the plastic bag before you remove it. Hold the bag together at the top and use a cord to tie up the bag.