# Assembly

- Pull the plug out of the socket before cleaning or performing maintenance on the vacuum cleaner, making tool adjustments, changing accessories or putting away the vacuum cleaner. This safety measure prevents the vacuum cleaner from being started accidentally.

Fitting the vacuuming accessories
Fitting the Vacuum Hose
Inserting/Removing the Plastic Bag (Dry Extraction)
Inserting/Removing the Fleece Filter Bag (Dry Extraction)
Attaching the L-BOXX
Installing the Retractable Guide Handle (Accessory)