# Technical data

Wet/dry extractor |  | GAS 400 A | GAS 400 A
--- | --- | --- | ---
Article number ‎3 601 JM0 ...‎‎‎‎ |  | ‎... 020/... 0F0‎ ‎... 080/... 0E0/... 0N0‎ ‎... 0K0‎ ‎... 0L0/... 070‎ ‎... 0H0‎ ‎... 030‎ | ‎... 0D0/... 0G0‎ ‎... 0C0‎ ‎... 060‎
Rated power input | W | 1200 | 1200
Frequency | Hz | 50–60 | 60
Container volume (gross) | l | 40 | 40
Net volume (dry) | l | 28 | 26
Net volume (liquid) | l | 20 | 18
Vacuum pressureA) |
Dust extractor | hPa | 200 | 180
Turbine | hPa | 230 | 200
Flow rateA) |
Dust extractor | l/s m3/h | 28 100,8 | 26 93,6
Turbine | l/s m3/h | 71,5 257 | 70 252
Dust class |  | L | L
WeightB) | kg | 14,0 | 14.5
Protection class |  | /I | /I
Protection rating |  | IPX4 | IPX4

A)

  Measured using a vacuum hose 4 m long and 28 mm in diameter

B)

  Weight without mains connection cable and without mains plug

The specifications apply to the specified rated voltages. These specifications may vary at different voltages and in country-specific models.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.

## Plug socket on the dust extractor

Permitted connected load of the connected power tool
‎3 601 JM0 …‎‎‎ | Rated voltage | Maximum power | Minimum power
--- | --- | --- | ---
‎... 020/... 0F0‎ | 230 V | 2100 W | 100 W
‎... 080/... 0E0/... 0N0‎ | 220 V | 2100 W | 100 W
‎... 0K0‎ | 220−230 V | 2100 W | 100 W
‎... 0L0/... 070‎ | 220−240 V | 1660 W | 100 W
‎... 0H0‎ | 220 V | 1000 W | 100 W
‎... 030‎ | 230 V | 1100 W | 100 W
‎... 0D0/... 0G0‎ | 127 V | 705 W | 100 W
‎... 0C0‎ | 115 V | 525 W | 100 W
‎... 060‎ | 110 V | 560 W | 100 W

Permitted connected load of the connected power tool.
These values can differ for other country-specific models. Please take note of the information on the socket of the dust extractor.