# Status Indicators

Status indicator (4) | Meaning
--- | ---
After Tapping the On Switch:
0.5 s illuminated green | Power tool ready for use
3 s illuminated red | Battery is too weak for pressing process, replace battery
Battery outside the operating temperature, allow battery to reach the correct temperature
When the On Switch is Pressed:
Illuminated red | Internal error Send the power tool to an authorised Bosch after-sales service centre for maintenance.
After the Pressing Process:
3 s illuminated green | Maximum pressing force reached during pressing process
3 s illuminated red | Pressing process is not completed
Continuous:
Illuminated yellow | 40000 work cycles reached Send the power tool to an authorised Bosch after-sales service centre for maintenance.