# Technical Data

Pressing machine | GPT 18V‑19 | GPT 18V‑32
--- | --- | ---
Article number |  | ‎3 601 JM2 000‎‎‎‎ | ‎3 601 JM2 100‎‎‎‎
Rated voltage | V | 18 | 18
Max. pressing force Fmax | kN | 21 | 34
Pressing timeA) | s | 3 | 5
Tool holder turning range | ° | 360 | 360
Pressing area
Max. diameter of plastic pipesB) | mm | 40 | 110
Max. diameter of metal pipes | mm | 35 | 54
WeightC) | kg | 2.5 | 3.4
Dimensions (lengthD) × width × height) | mm | 395 × 105 × 150 | 486 × 105 × 136
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35
Permitted ambient temperature during operation | °C | +5 to +50 | +5 to +50
Permitted ambient temperature during storage | °C | −20 to +50 | −20 to +50
Compatible rechargeable batteries (2.0−8.0 Ah) |  | GBA 18V… ProCORE18V… EXPERT18V… EXBA18V… CORE18V… | GBA 18V… ProCORE18V… EXPERT18V… EXBA18V… CORE18V…
Recommended battery chargers |  | GAL 18V… GAL 36V… GAL 12V/18… GAX 18V… EXAL18V… | GAL 18V… GAL 36V… GAL 12V/18… GAX 18V… EXAL18V…

A)

  measured with press jaw SV18 or SV28

B)

  Fittings of 110 mm can only be pressed with rechargeable batteries with a capacity of at least 4.0 Ah.

C)

  without battery, without press jaw (you can find the battery weight on www.bosch-professional.com.)

D)

  with a screwed-in tool holder

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.