# Technical data

Circular saw |  | GKS 18V-44 | GKS 18V-51
--- | --- | --- | ---
Article number |  | ‎3 601 JM3 0..‎ | ‎3 601 JM3 1..‎
Rated voltage | V | 18 | 18
Rated no-load speedA) | min–1 | 6300 | 6300
Max. cutting depth
at a 0° mitre/bevel angle | mm | 44 | 51
at a 45° mitre/bevel angle | mm | 30 | 35
Spindle lock |  | ● | ●
Base plate dimensions | mm | 117 x 222 | 117 x 230
Saw blade diameter | mm | 125 | 140
Max. base blade thickness | mm | 1.8 | 1.8
Min. base blade thickness | mm | 0.6 | 0.6
Locating bore | mm | 20 | 20
Weight according to EPTA-Procedure 01:2014B) | kg | 2.4–3.5 | 2.5–3.6
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50 | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ≥ 4.0 Ah ProCORE18V... ≥ 4.0 Ah | GBA 18V... ≥ 4.0 Ah ProCORE18V... ≥ 4.0 Ah
Recommended chargers |  | GAL 18... GAX 18... GAL 36... | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 4.0Ah

B)

  Depending on battery in use

C)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.