# Inserting the application tool (see figures A–B)

##

## GDR 18V-215:

NOTE: Depending on the article number, only certain types of bits can be used (see table below).

GDR 18V-215: | ‎3 601 JN2 020 ‎3 601 JN2 0E0 ‎3 601 JN2 040 | ‎3 601 JN2 0L0 ‎3 601 JN2 050
Single end bit | 9.5 mm | 9.5 mm 14 mm
Double end bit | 9.8 mm | 9.8 mm 17 mm

Pull the locking sleeve (2) forward, guide the application tool (1) into the tool holder up to the stop and release the locking sleeve (2) to lock the application tool.

Screwdriver bits (13) can be inserted using a universal bit holder with ball catch (12).

##

- Observe the information on the safe use of application tools. Some application tools are not suitable for this power tool due to the high torque.

- When fitting an application tool, make sure that it is held securely in the tool holder. If the application tool is not held securely in the tool holder, it may become loose and consequently uncontrollable.

NOTE: Depending on the article number, only certain types of bits can be used (see table below).

GDX 18V-285: | ‎3 601 JN2 120 ‎3 601 JN2 1E0 | ‎3 601 JN2 1L0 ‎3 601 JN2 150
Single end bit | 9.5 mm | 9.5 mm 14 mm
Double end bit | 9.8 mm | 9.8 mm 17 mm

Slide the application tool (14) onto the square drive of the tool holder (1).

Due to the way the system operates, the application tool (14) will move around slightly in the tool holder (1); this has no influence on the function/safety.

##

Pull the locking sleeve (2) forward and remove the application tool.