# Technical Data

Cordless Impact Screwdriver |  | GDR 18V-215 | GDX 18V-285
--- | --- | --- | ---
Article number |  | ‎3 601 JN2 0..‎ | ‎3 601 JN2 1..‎
Rated voltage | V= | 18 | 18
No-load speed
Setting 1 | min–1 | 2100A) | 2000B)
Setting 2 | min–1 | 3300A) | 2800B)
Impact rate
Setting 1 | min–1 | 3000A) | 3000B)
Setting 2 | min–1 | 3800A) | 3600B)
Max. tightening torque | Nm | 215A) | 285B)
Max. loosening torque | Nm | – | 500B)
Machine screw diameter | mm | M6–M16 | M8–M18
Tool holder |  | ¼" internal hexagon | ½" external square ¼" internal hexagon
WeightC) | kg | 1.4–2.4 | 1.5–2.5
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35
Permitted ambient temperature during operationD) and during storage | °C | –20 to +50 | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V... | GBA 18V... ProCORE18V...
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36... | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 4.0Ah

B)

  Measured at 20–25 °C with rechargeable battery ProCORE18V 12.0Ah

C)

  Depending on battery in use

D)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.