# Switching on/off

To start the power tool, press and hold the on/off switch (9).

The worklight (3) lights up when the on/off switch (9) is lightly or fully pressed, allowing the work area to be illuminated in poor lighting conditions.

To switch off the power tool, release the on/off switch (9).

The worklight (3) will remain lit for approx. 15 seconds after the on/off switch (9) has been released.