# Technical Data

Battery Charger | GAL 1880 CV
--- | ---
Protection class | / II
Charging currentA) | 8.0 A
Battery charging voltage (automatic voltage detection) | 14.4–18 V
WeightB) | 0.66 kg

A)

  Depends on temperature and rechargeable battery type

B)

  Weight without mains connection cable and without mains plug

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.