# Start-Up

## Switching on/off

To start the power tool, push the on/off switch (3) forward.

To lock the on/off switch (3) in position, push the on/off switch (3) forward and down until it clicks into place.

To switch off the power tool, release the on/off switch (3); or, if the switch is locked, briefly push the on/off switch (3) backward and down and then release it.

- Always check abrasive tools before using them. The abrasive tool must be fitted properly and be able to move freely. Carry out a test run for at least one minute with no load. Do not use abrasive tools that are damaged, run untrue or vibrate during use. Damaged abrasive tools can burst apart and cause injuries.