# Switching on/off

Note: Unlock the on/off switch (8) by pushing the lock-off button (9) upwards (see figure D).

To start the power tool, press and hold the on/off switch (8).

The worklight (10) lights up when the on/off switch (8) is lightly or fully pressed, allowing the work area to be illuminated in poor lighting conditions.

To switch off the power tool, release the on/off switch (8).

Note: Once work is complete, lock the on/off switch (8) by pushing the lock-off button (9) downwards (see figure D).