# Technical Data

Cordless ratchet wrench |  | GRC 18V-60
--- | --- | ---
Article number |  | ‎3 601 JN8 0..‎
Rated voltage | V= | 18
No-load speedA) | min–1 | 400
Max. torqueA) | Nm | 60
Max. screw diameter | mm | M12
Tool holder |  | ∎ 3/8"
WeightB) | kg | 1.3–2.4
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V...
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 2.0Ah

B)

  Measured with GBA 18V 1.5Ah and GBA 18V 12Ah.

C)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.