# Switching on/off

Note: Unlock the on/off switch (7) by pushing the lock-off button (8) upwards (see figure C).

To start the power tool, press and hold the on/off switch (7).

The worklight (9) lights up when the on/off switch (7) is lightly or fully pressed, allowing the work area to be illuminated in poor lighting conditions.

To switch off the power tool, release the on/off switch (7).

Note: Once work is complete, lock the on/off switch (7) by pushing the lock-off button (8) downwards (see figure C).