# Technical Data

Cordless ratchet wrench |  | GRC 12V-60 1/2 SN | GRC 12V-60 3/8 SN
--- | --- | --- | ---
Article number |  | ‎3 601 JN8 5..‎ | ‎3 601 JN8 3..‎
Rated voltage | V= | 12 | 12
No-load speedA) | min-1 | 0–230 | 0–230
Max. torque, hard screwdriving application according to ISO 5393A) | Nm | 60 | 60
Max. screw diameter | mm | M12 | M12
Tool holder |  | ∎ 1/2" | ∎ 3/8"
WeightB) | kg | 0.97–1.16 | 0.95–1.14
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50 | –20 to +50
Recommended rechargeable batteries |  | GBA 12V... | GBA 12V...
Recommended battery chargers |  | GAL 12... GAX 18... | GAL 12... GAX 18...

A)

  Measured at 20–25 °C with rechargeable battery GBA 12V 2.0 Ah

B)

  Depending on battery in use

C)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.