# Setting the Rotational Direction (see figure B)

- The head of the ratchet wrench and the rotational direction switch can become hot during operation. There is a risk of burns in the event of contact. Allow the ratchet wrench to cool.

The rotational direction switch (2) is used to change the rotational direction of the power tool. However, this is not possible while the on/off switch (7) is being pressed.

Clockwise: To drive in screws and tighten nuts, turn the rotational direction switch (2) anticlockwise.

Anti-clockwise rotation: To loosen or unscrew screws and nuts, turn the rotational direction switch (2) clockwise.