# Operation

- Pull the plug out of the socket before carrying out any work on the power tool.

- Products that are only sold in AUS and NZ: Use a residual current device (RCD) with a nominal residual current of 30 mA or less.

Transport safety lock
Locking the Glide Arm
Preparing for operation
Adjusting the Mitre Angle
Adjusting Bevel Angles
Start-up
Practical advice
Sawing
Working on mouldings
Checking and Adjusting the Basic Settings
Transport