# Fitting individual components

- Carefully remove all parts included in the delivery from their packaging.
- Remove all packing material from the power tool and the accessories provided.

## Fitting the locking knob (see figure a)

- Screw the locking knob (11) into the corresponding hole above the lever (12).

- Always tighten the locking knob (11) firmly before sawing. Otherwise the saw blade can become wedged in the workpiece.