# Start-up

- Pay attention to the mains voltage. The voltage of the power source must match the voltage specified on the rating plate of the power tool.

##

- To switch on the power tool, first slide the lock-off button (2) to the middle and then press and hold the on/off switch (58).

Note: For safety reasons, the on/off switch (58) cannot be locked; it must remain pressed during the entire operation.

##

- To switch off, release the on/off switch (58).

##

The electronic starting current limitation restricts the power consumption when the power tool is switched on and enables operation with a 16 A fuse.

Note: If the power tool runs at full speed immediately after being switched on, this means that the starting current limitation and restarting protection mechanisms have failed. The power tool must be sent to the after-sales service without delay.