# Technical Data

Sliding Mitre Saw |  | GCM 12 GDL | GCM 12 GDL | GCM 12 GDL | GCM 12 GDL
--- | --- | --- | --- | --- | ---
Article number |  | ‎3 601 M23 60.‎ ‎3 601 M23 63.‎ ‎3 601 M23 67.‎ | ‎3 601 M23 66.‎ | ‎3 601 M23 64.‎ | ‎3 601 M23 6B.‎
Rated power input | W | 2000 | 1500 | 2000 | 1800
Rated voltage | V | 230–240 | 110 | 230–240 | 220
Frequency | Hz | 50/60 | 50/60 | 50 | 60
No-load speed | min–1 | 4000 | 4000 | 4000 | 4000
Starting current limitation |  | ● | – | ● | ●
Laser type | nm | 650 | 650 | 650 | 650
| mW | < 0.39 | < 0.39 | < 0.39 | < 0.39
Laser class |  | 1 | 1 | 1 | 1
WeightA) | kg | 29.4 | 29.4 | 29.4 | 29.4
Protection class |  | / II | / II | / II | / II
Dimensions of suitable saw blades |
Saw blade diameter D | mm | 305 | 305 | 305 | 305
Base blade thickness | mm | 1.7–2.6 | 1.7–2.6 | 1.7–2.6 | 1.7–2.6
Max. cutting width | mm | 3.2 | 3.2 | 3.2 | 3.2
Hole diameter d | mm | 30 | 30 | 25.4 | 25.4

A)

  Weight without mains connection cable and without mains plug

Permissible workpiece dimensions see Permissible workpiece dimensions

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.