# Product features

The numbering of the product features refers to the diagram of the power tool on the graphics page.

(1) | Handle
(2) | Lock-off button for on/off switch
(3) | Protective guard
(4) | Retracting blade guard
(5) | Adjustable fence
(6) | Fence
(7) | Saw table extension
(8) | Mounting holes
(9) | Insert plate
(10) | Locking clamp
(11) | Locking knob for all mitre angles
(12) | Mitre pre-setting lever
(13) | Clamping handle for all bevel angles
(14) | Detents for standard mitre angles
(15) | Recessed handles
(16) | Hex key (6 mm/4 mm)
(17) | Hex key (2 mm)
(18) | Screw clamp
(19) | Guide roller
(20) | Angle indicator for right-hand bevel angle range (0° to 47°)
(21) | Chip deflector
(22) | Chip ejector
(23) | Dust extraction adapter
(24) | Glide mechanism clamping lever
(25) | Laser warning label
(26) | Laser protection cap
(27) | Glide arm
(28) | Depth stop adjusting screw
(29) | Depth stop
(30) | Transport safety lock
(31) | Scale for bevel angles
(32) | Angle indicator for left-hand bevel angle range (47° to 0°)
(33) | Adjustment knob for 22.5° bevel angle
(34) | Locking screw for length stop
(35) | Length stop
(36) | Scale for mitre angles
(37) | Saw table
(38) | Rotary knob for adjusting the bevel angle range
(39) | Saw blade
(40) | Laser beam outlet aperture
(41) | Locking screw for the linkage of the retracting blade guard
(42) | Linkage of the retracting blade guard
(43) | Front fastening screw (cover plate/retracting blade guard)
(44) | Rear fastening screw (cover plate/retracting blade guard)
(45) | Cover plate
(46) | Spindle lock
(47) | Hex socket screw for mounting the saw blade
(48) | Clamping flange
(49) | Inner clamping flange
(50) | Clamping lever of the saw table extension
(51) | Locking screw for the adjustable fence
(52) | Damper
(53) | Set screws for damping
(54) | Holes for screw clamp
(55) | Wing bolt
(56) | Threaded rod
(57) | Angle indicator for mitre angles
(58) | On/off switch
(59) | On/off switch for laser (cutting line indication)
(60) | Screws for insert plate
(61) | Clamping screw for length stop
(62) | Screw for laser protection cap
(63) | Set screw for positioning the laser (flush levelling)
(64) | Fastening screw for laser mounting plate
(65) | Fastening screw for laser housing
(66) / (67) / (68) | Set screws for 0° basic setting (bevel angle)
(69) | Set screw for 45° basic setting (left-hand bevel angle)
(70) | Set screw for 45° basic setting (right-hand bevel angle)
(71) | Set screws for mitre angle scale
(72) | Screw for mitre angle indicator
(73) | Set screw for adjusting the clamping force of the clamping handle for any bevel angle
(74) | Hook-and-loop strap