# Transport (see figure Z)

Before transporting the power tool, the following steps must be carried out:

- Slide the glide arm (27) all the way back and secure it in this position.
- Make sure that the depth stop (29) is pressed all the way in and that the adjusting screw (28) fits through the recess without touching the depth stop when moving the glide arm.
- Guide the glide arm downwards until you can press the transport safety lock (30) all the way in
- Slide the saw table extensions (7) all the way in.
- Set the bevel angle to 0° and tighten the clamping handle (13).
- Turn the saw table (37) as far as possible to the left and tighten the locking knob (11).
- Wind up the mains cable and tie it together with the hook-and-loop strap (74).
- Remove all accessories that cannot be securely fitted to the power tool.
- If possible, transport unused saw blades in an enclosed container.
- For transport, hold the power tool by the recessed handles (15) on either side of the saw table.

- When transporting the power tool, only use the transport fixtures. Never carry the power tool by the protective devices, the glide arm or the handle.