# Locking the Glide Arm

The glide mechanism of the glide arm (27) can be locked with the clamping lever (24). The glide arm can be placed in two positions:

- Glide arm pushed all the way back (for cross cuts)
- Glide arm pulled all the way forward (for a compact transport position)

## Unlocking the Glide Arm (see figure B1)

After unlocking the glide arm (27), the whole gliding mechanism is ready for operation.

- Press the clamping lever (24) all the way down.
- The clamping wedge of the clamping lever releases the two articulated parts at the bottom of the glide arm.

## Securing the Glide Arm (see figure B2)

Glide arm pushed all the way back:

- Push the glide arm (27) all the way back.
- The two articulated parts at the top of the glide arm are now upright and closed.
- Pull the clamping lever (24) upwards until the clamping wedge is positioned between the two articulated parts at the bottom of the glide arm.
- This locks the glide arm (27), which is pushed all the way back.

Glide arm pulled all the way forward:

- Pull the glide arm (27) all the way forward.
- The glide mechanism is now completely extended.
- Pull the clamping lever (24) upwards until the clamping wedge is positioned between the two articulated parts at the bottom of the glide arm.
- This locks the glide arm (27), which is pulled all the way forward.