# Transport Safety Lock (see figure A)

The transport safety lock (30) makes it easier to handle the power tool when transporting it to various working locations.

## Unlocking the Power Tool (Work Position)

- Press the glide arm (27) down slightly by the handle (1) to release the transport safety lock (30).
- Pull the transport safety lock (30) all the way out.
- Slowly guide the glide arm (27) upwards.

## Locking the Power Tool (Transport Position)

- Slide the glide arm (27) all the way back and secure it in this position.
- Guide the glide arm downwards until you can press the transport safety lock (30) all the way in.

Further information: see Transport (see figure Z)